## Pan & Tilt – Ordering Options

## Customer:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Type** |  |  | KPA-45 | Pan unit, single axis |
|  |  |  | KPT-45 | Pan-Tilt unit, dual axis |
|  |  |  |  |  |
| **Housing material** |  |  | AL | Aluminum Housing (Hard Anodized) |
|  |  |  | TI | Titanium Housing |
|  |  |  |  |  |
| **Gear Ratio** |  |  | 1:120 | Standard gear ratio |
|  |  |  | 1:160 | Higher torque, less speed |
|  |  |  |  |  |
| **Accuracy** |  |  | S | Standard ± 0.1° (0.1° resolution) |
|  |  |  | H | High ± 0.01° (0.001° resolution), on request |
|  |  |  |  |  |
| **Command interface** |  |  | RS-232 | RS-232, 115200 Baudrate |
|  |  |  | RS-485 | RS-485, 2 wire, 115200 Baudrate |
|  |  |  | Ethernet | 100 Mbps Ethernet, (depth 1000m) on request |
|  |  |  |  |  |
| **Compensator** |  |  | E | External compensator interface |
|  |  |  | I | Internal compensator (with Flared JIC 37° Fitting only) |
|  |  |  |  |  |
| **Compensator interface** |  |  | FL | Flared JIC 37° Fitting |
|  |  |  | BS | BS 1/8” BSPP Tread |
|  |  |  | BP | PB4 hose |
|  |  |  | Others:  please specify |  |
|  |  |  |  |  |
| **Pigtail connector** |  |  | SE | Seacon, Micro Wet-Con series, MCBH5MSS |
| **at unit** |  |  | Others:  please specify |  |
|  |  |  |  |  |
| **Pigtail cable length** |  |  | 0.6 m |  |
|  |  |  | Other lengths:  please specify |  |
|  |  |  |  |  |
|  |  |  |  |  |
| **Additional requirements:**  **Please specify** |  | | | |